
To update a SC4200c instrument, you can follow the standard procedure: 
-	extract from .zip file the 'update' folder to a USB stick root,
-	plug it to the (running) SC42000c device you want to update,
-	wait for the end of update: USB flashing / probes amber waving / reboot (all LED off / normal start).


Note:
The open-source code used in that device can be found at https://github.com/HachCompany-SC4200/
Instructions on how to build the device can be found at https://github.com/HachCompany-SC4200/fusion_seacloud_platform/blob/github_publication_SC4200/README.md
The related open-source licenses can be found at https://github.com/HachCompany-SC4200/fusion_licenses


